Version

FCar Reader F502 upgrade unitity
Version 1.0 release, May,2013
Version 2.0 release, May,2014
Version 3.0 release, August, 2015
 
Introduction
 
Product Description
 
F502 is a palm size handheld heavy duty truck code reader/scanner who is latest developed by FCar Tech. It is 2.8 inch LCD true color display with 320x240 pixel and can support heavy duty truck standard protocols J1939 and J1708. It covers Cummings, Detroit, FUSO, HINI, MAN, Caterpillar, Freightliner, International, Kenworth, John Deere, Peterbilt, Sterling, Iveco ISUZu, JAC, Mack, Mecedes Benz, NISSAN, SCANIA, VOLVO and more diesel trucks, buses and engines whoever are supported by J1939 or J1708. This high quality and performance scanner is ideal for heavy futy truck/bus owner or truck fleet dignostic professional.
 
Product Information
1.Scan heavy-duty trucks by J1939 or J1708
2.Scan truck ECU components to read all DTC, clear Code and show live data stream.
3.The components are including Engine, Transmission, Brake, Turbocharger, Axle, Power unit, Trailer, Instrument cluster and much more
4.OBD16 via Diesel 6 pin or Diesel 9 pin connectors
 
Installation Guide
 
[Windows XP/Vista]
1. vcom.inf is usb driver, Right click to install
2. Click FcarReader_502.exe to open update window
3. Select the driver COM, follow the window Instructions
 
[Windows 7]
 
1.Code reader power off or unplug USB cable
2.Press and hold the [Enter] button on the code reader, and plug in the USB cable into your pc
3.All three indicator lights on the code reader turn on, and release the button
4.Code reader enters into upgrade maintenance mode
5.Install USB Driver
	1)Click Windows Start menu-->Control Panel-->Device Manager
	2)Click to expand "F50x USB VCom Port (COM4)"
	3)Right click on Update Driver and Browse my computer for driver software
	4)Select vcom.inf from your download package
	6. Go back to Upgrade Unitity to Select the serial port ([Query serial port] button to update the current serial port list and select new port [COM4]
	7. Click [Start Upgrade]

 
[Windows 8/Windows 10]
 
How To Disable Driver Signature Enforcement In Windows 8/8.1 And Windows 10
Find PC Settings from the start menu or apps list >> select Update and Recovery >> click Recovery.
Under Advanced Startup, click on Restart Now.
Your PC will do a kind of reboot and go to a blue Choose an option screen. Click on Troubleshoot (refresh or reset your PC or use advanced tools) >> Advanced Options >> Startup Settings (change windows startup behaviour) >> Restart.
Your PC will now restart and go to yet another blue screen with 10 options. Press 7 or F7 on your keyboard to select Disable driver signature enforcement.
Your computer will auto restart again and then you can now proceed with the installation of FCAR F502 USB VCOM driver for Windows 7/8/8.1/10.